FlyByWire A380X Checklist

For simulation purposes only

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BEFORE START** | |  | **APPROACH** | |
| SECURITY INSPECTION | COMPLETE |  | CABIN CREW | ADVISE |
| CKPT PREP | COMPLETE |  | LANDING DATA | SET |
| OXYGEN | \_\_ SET |  | AUTO BRAKE/BTV | AS RQRD |
| GEAR PINS & COVER | REMOVE |  | LANDING BRIEFING | CONFIRM |
| FUEL QTY | \_\_ LBS +/- \_\_ LBS |  | ECAM STS | NORMAL |
| T.O DATA | SET |  | ALTIMETER | \_\_ QNH/HPA SET |
| ALTIMETER | \_\_ INHG/HPA SET |  | LAND SW | **ON** |
| PARK BRK | SET |  | MINIMA | SET |
| SIGNS | ON/AUTO |  | SEAT BELTS | ON |
| WINDOWS/DOORS | CLOSE |  |  |  |
| BEACON | ON |  | **LANDING** | |
|  |  |  | A/THR MODE | AS RQRD |
| **AFTER START** | |  | SIGNS | ON |
| A-ICE | AS RQRD |  | LDG GEAR | DOWN |
| F/CTL | CHECK |  | FLAPS | LDG |
| RUDDER TRIM | NEUTRAL |  | SPLRs | ARM |
| PITCH TRIM | CHECK |  |  |  |
| GROUND EQUIPMENT | CLEAR |  | **AFTER LANDING** | |
|  |  |  | EXTERIOR LIGHTS | SET |
| **BEFORE TAKEOFF** | |  | SPLRs | DISARM |
| FLIGHT INSTRUMENTS | CHECK |  | FLAPS | 0 |
| TAKEOFF BRIEFING | CONFIRM |  | APU | START |
| V1/VR/V2/FLEX TEMP | CHECK |  |  |  |
| SIGNS | ON |  | **PARKING** | |
| SPLRs | ARM |  | PARK BRK | ON |
| FLAPS | T.O |  | EXT LT | AS RQRD |
| AUTO BRAKE | RTO |  | APU BLEED | ON |
| T.O CONFIG | NORMAL |  | ALL ENGs | OFF |
| CABIN CREW | READY |  | FUEL PMPs | OFF |
| PACK 1+2 | AS RQRD |  | SEAT BELTS | OFF |
| EXTERIOR LIGHTS | SET |  |  |  |
|  |  |  | **SECURING THE AIRCRAFT** | |
| **AFTER TAKEOFF/CLIMB** | |  | ADIRS | OFF |
| LDG GEAR | UP |  | OXYGEN | OFF |
| FLAPS | 0 |  | APU BLEED | OFF |
| PACK 1+2 | ON |  | EMER EXIT LT | OFF |
| APU MASTER SW | OFF |  | SIGNS | OFF |
| LAND SW | OFF |  | APU | OFF |
| ALTIMETER | STANDARD SET |  | ALL 3 LAPTOPS | OFF |
|  |  |  | ALL 4 BATs | OFF |